**EAST CENTRAL ARKANSAS REGIONAL LIBRARY
REQUEST FOR BIDS**

The Cross County Library, a unit of the East Central Arkansas Regional Library is accepting bids for one

**COMPACT 6-7 PASSENGER MINI-VAN**

until Noon on Friday, April 15, 2022 in the office of the Regional Librarian.

Bids must be submitted on the attached specification and bid document sheet. Bids are to be submitted in writing, to the Regional Librarian, ATTN: TRUCK BID, 410 Merriman Avenue, East, Wynne, Arkansas 72396. Bids may be submitted via email to jpaul@ecarls.org. Bids will not be accepted via telephone or fax. Bids must be in hand by the date specified – postmarked but not delivered bids will be rejected. Management reserves the right to reject any and all bids.

In lieu of new vehicles, the Library will consider used vehicles meeting specifications not more than 2 years old with not less than 5,000 nor more than 10,000 miles prior use. A purchase of a used motor vehicles, equipment or machinery shall be accompanied by a statement in writing from the vendor on the bill of sale or other document that the motor vehicle, equipment, or machinery is at least 1 year in age from the date of original manufacture or has been used a minimum of 250 hours or driven a minimum of 5000 miles.

This unit is being purchased to provide mobile library services within the library region. In addition to meeting library service deficits, the unit will provide ample promotional and marketing opportunities for the library and for supporters.

Questions may be submitted to the Regional Librarian at jpaul@ecarls.org.

|  |  |  |
| --- | --- | --- |
|  | **Dealer Name:** | **RED RIVER DODGE CHYSLER JEEP RAM** |
|  | **Vehicle Make/Model/Year:** | **CHRYSLER VOYAGER LX** |
| **Minivan 2WD, 6-7 Passengeras classified in the latest EPA Fuel Economy Guide** | **Model Code:** | **RUCE53** |
| **City MPG Estimate:** | **19** |
| **Highway MPG Estimate:** | **22** |
|  | **One Way Delivery Charge Per Mile:** | **1.50 PER MILE**  |
|  | **VEHICLE BID PRICE:** | **$27,205.00** |
| **Body & Chassis** | **Base Vehicle Minimum Requirements** | **Enter Vehicle Specification and Manufacturer Codes (Fill-in Unshaded Blanks Only)** |
| Mini-Van 6-7 Passenger | Mini-Van 7 Passenger |   |
| Interior Volume | Combined interior volume (passenger and cargo) 180 cubic feet |   |
| **Engine** |   |   |
| Engine Size  | 260 hp - List HP, Liters & Cylinders | 3.6L V6 287 HP |
| Fuel Type | Gasoline |   |
| **Transmission/Drivetrain** |   |   |
| Automatic Transmission | Automatic or CVT - List Type, Speeds etc. | AUTO 9 SP |
| 2WD | 2WD  |   |
| Electronic Stability Control | Electronic Stability Control System |   |
| Differential Type/Ratio | Mfg.Std. - List Ratio & Type |   |
| **Electrical** |   |   |
| Alternator | Mfg. Std.  |   |
| Battery  | Mfg. Std.  |   |
| Power Outlet | 12 -Volt Power Outlet |   |
| Daytime Running Lights | Mfg. Std.  |   |
| **Fuel Tank** |  |  |
| Fuel Capacity (Gals) | Mfg. Std. - List Amount in Gallons | 19 |
| **Exterior** |  |  |
| Paint | White |   |
| Bumpers | Mfg.Std Front & Rear |   |
| License Plate Brackets | Front and Rear Brackets |   |
| Windshield Washer | Windshield Washer & Multi-Speed Wipers |   |
| **Doors & Mirrors** |  |  |
| Doors  | 5 doors, two passenger, two sliding, one rear liftback |   |
| Mirrors | Two Outside, Right & Left, One inside |   |
| **Interior** |  |  |
| Air Conditioning | AC Factory Installed |   |
| Radio | Audio system with AM/FM Stereo, Bluetooth, LCD Multi-Function Display plus 1 USB Port |   |
| Cruise | Cruise Control, Factory Installed  |   |
| Tilt Steering | Tilt Steering Wheel |   |
| Steering | Power Steering |   |
| Windows | Mfg. Standard |   |
| Power Windows & Door Locks | Power Windows & Door Locks |   |
| Tinted Glass | Mfg. Std. Tint on All Windows |   |
| Floor Mats | Front & Rear, Color to Match Interior |   |
| **Seats** |  |  |
| Seats | Mfg. Std., Colors Must Blend With InteriorExterior Color  |   |
| **Safety** |  |  |
| Brakes | Anti-Lock Brake System (ABS) - List Disc/Drums | ABS 4 WH DISC |
| Restraint System All Pass | Required |   |
| Air Bags, Front, Both Sides | Required |   |
| **Towing** |   |   |
| Towing Package | Mfg. Standard |   |
| **Tires & Wheels** |  |  |
| Tires & Wheels | Mfg. Std. - List Size | P235/65R17 |
| Spare | Mfg. Std. List  | TIRE KIT |
| **Warranty** |  |  |
| Bumper to Bumper Warranty | 3 Years or 36,000 miles, whichever comes first  |   |
| Drive Train Warranty | List Warranty | 5YR/100K MILES  |